# Static Call Graph for image .\STM32F1_SUART.axf

#<CALLGRAPH># ARM Linker, 5060300: Last Updated: Wed May 08 08:36:54 2019

### Maximum Stack Usage = 0 bytes

### Call chain for Maximum Stack Depth:

### Global Symbols

CPSID (Thumb, 4 bytes, Stack size 0 bytes, stm32f1_suart.o(.emb_text), UNUSED)
[Called By]

- >> WriteUART
- >> ReadUART

CPSIE (Thumb, 4 bytes, Stack size 0 bytes, stm32f1_suart.o(.emb_text), UNUSED)
[Called By]

- >> WriteUART
- >> ReadUART

InitUART (Thumb, 54 bytes, Stack size 16 bytes, stm32f1_suart.o(.text), UNUSED)
[Called By]

- >> Run

Delay (Thumb, 6 bytes, Stack size 0 bytes, stm32f1_suart.o(.text), UNUSED)
[Calls]

- >> Delay

[Called By]

- >> Delay

ReadUART (Thumb, 90 bytes, Stack size 24 bytes, stm32f1_suart.o(.text), UNUSED)
[Calls]

- >> CPSIE
- >> CPSID

[Called By]

- >> ReadUART32

WriteUART (Thumb, 86 bytes, Stack size 32 bytes, stm32f1_suart.o(.text), UNUSED)
[Calls]

- >> CPSIE
- >> CPSID

[Called By]

- >> WriteUART32

ReadUART32 (Thumb, 68 bytes, Stack size 24 bytes, stm32f1_suart.o(.text), UNUSED)
[Calls]

- >> ReadUART

[Called By]

- >> TestUART

WriteUART32 (Thumb, 100 bytes, Stack size 24 bytes, stm32f1_suart.o(.text), UNUSED)
[Calls]

- >> WriteUART

[Called By]

- >> TestUART

TestUART (Thumb, 32 bytes, Stack size 16 bytes, stm32f1_suart.o(.text), UNUSED)
[Calls]

- >> WriteUART32
- >> ReadUART32

[Called By]

- >> Run

Run (Thumb, 30 bytes, Stack size 8 bytes, stm32f1_suart.o(.text), UNUSED)
[Calls]

- >> TestUART
- >> InitUART

### Local Symbols

### Undefined Global Symbols