# Static Call Graph for image C:\JM3\JM3_Plguin\XMC1000\XMC1000_SUART.axf

#<CALLGRAPH># ARM Linker, RVCT4.0 [Build 524]: Last Updated: Wed May 08 08:49:27 2019

### Maximum Stack Usage = 0 bytes

### Call chain for Maximum Stack Depth:

### Global Symbols

CPSID (Thumb, 4 bytes, Stack size 0 bytes, xmc1000_suart.o(.emb_text), UNUSED)
[Called By]

- >> WriteUART
- >> ReadUART

CPSIE (Thumb, 4 bytes, Stack size 0 bytes, xmc1000_suart.o(.emb_text), UNUSED)
[Called By]

- >> WriteUART
- >> ReadUART

InitUART (Thumb, 54 bytes, Stack size 16 bytes, xmc1000_suart.o(.text), UNUSED)
[Called By]

- >> Run

Delay (Thumb, 6 bytes, Stack size 0 bytes, xmc1000_suart.o(.text), UNUSED)
[Calls]

- >> Delay

[Called By]

- >> Delay

ReadUART (Thumb, 88 bytes, Stack size 24 bytes, xmc1000_suart.o(.text), UNUSED)
[Calls]

- >> CPSIE
- >> CPSID

[Called By]

- >> ReadUART32

WriteUART (Thumb, 80 bytes, Stack size 32 bytes, xmc1000_suart.o(.text), UNUSED)
[Calls]

- >> CPSIE
- >> CPSID

[Called By]

- >> WriteUART32

ReadUART32 (Thumb, 70 bytes, Stack size 24 bytes, xmc1000_suart.o(.text), UNUSED)
[Calls]

- >> ReadUART

[Called By]

- >> TestUART

WriteUART32 (Thumb, 100 bytes, Stack size 24 bytes, xmc1000_suart.o(.text), UNUSED)
[Calls]

- >> WriteUART

[Called By]

- >> TestUART

TestUART (Thumb, 32 bytes, Stack size 16 bytes, xmc1000_suart.o(.text), UNUSED)
[Calls]

- >> WriteUART32
- >> ReadUART32

[Called By]

- >> Run

Run (Thumb, 28 bytes, Stack size 8 bytes, xmc1000_suart.o(.text), UNUSED)
[Calls]

- >> TestUART
- >> InitUART

### Local Symbols

### Undefined Global Symbols